CAN Transmitter User Guide

Table of Contents

[2 Overview 2](#_Toc24620486)

[3 Required Files and BOM 2](#_Toc24620487)

[3.1 Enclosure Models 2](#_Toc24620488)

[3.2 BOM 2](#_Toc24620489)

[3.3 Arduino Sketch 2](#_Toc24620490)

[4 Configuration Environment Setup 3](#_Toc24620491)

[4.1 Install Arduino IDE 3](#_Toc24620492)

[4.2 Install mcp\_can Library 3](#_Toc24620493)

# Overview

The purpose of this CAN transmitter is to send cyclic CAN messages to DECUs undergoing testing. The user can configure the following parameters:

* Baud rate
* CAN ID type (11/29 bit)
* Number of CAN messages
  + CAN message IDs
  + CAN message DLCs
  + CAN message data
  + CAN message period

This CAN transmitter is intended to be easy to create, easy to program, and easy to configure.

# Required Files and BOM

## Enclosure Models

The CAN transmitter requires a custom enclosure, consisting of a box and lid. These two *.stl* files are to be 3D printed.

## BOM

The CAN transmitter is based off the *Arduino Uno* development board and the *Seeed Technology CAN BUS shield*.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Description** | **Manufacturer Part #** | **Qty** | **Price (USD)** | **Extended Price (USD)** |
| ARDUINO UNO SMD R3 ATMEGA328 | A000073 | 1 | 20.90 | 20.90 |
| CANBUS SHIELD V2 | 103030215 | 1 | 24.99 | 24.99 |
| CONN RCPT HSG 3POS | DT04-3P-L012 | 1 | 4.35 | 4.35 |
| LED 5MM BLUE CLR PANEL MOUNT | 5596001007F | 1 | 9.12 | 9.12 |
| LED 5MM GREEN CLR PANEL MOUNT | 5596201007F | 1 | 9.12 | 9.12 |
| RES 56 OHM 1/2W 5% CF MINI | CFM12JT56R0 | 2 | 0.10 | 0.20 |
| MACHINE SCREW PAN PHILLIPS 4-40 | R4-40X1/4 2701 | 2 | 0.63 | 1.26 |
| AC/DC WALL MOUNT ADAPTER 9V 5W | VEL05US090-US-JA | 1 | 6.50 | 6.50 |
| BUMPER SQU 0.812"L X 0.812"W BLK | SJ-5523 (BLACK) | 1 | 1.50 | 1.50 |
| USB CABLE TYPE A TO B 30CM BLACK | Seeed Technology Co., Ltd | 1 | 1.99 | 1.99 |
|  |  |  | **Total** | **79.93** |

Minor and optional materials, such as solder, heat shrink tubing, and grommets are not included.

## Arduino Sketch

The CAN transmitter uses an Arduino sketch.

# Configuration Environment Setup

## Install Arduino IDE

Download the *Windows Installer* from the link: <https://www.arduino.cc/en/Main/Software>

Install and run the *Arduino IDE*

## Install mcp\_can Library

Download the *mcp\_can* library by clicking the *Clone or Download* button. Follow the installation instructions in the *README.md* file.